**NOTES TO SPECIFIER:**

**Review and remove any text in RED before sending.**

**Edit options are typically flagged in the following manner:**

**EDIT – choices need decision or detailed review**

**NOTE – note to specifier regarding selection**

**OPTION – note when there may be an option for the article and/or paragraph**

**[font in brackets] = edit options for consideration**

SECTION 087114

POCKET DOOR HARDWARE

1. GENERAL
   * + 1. SUMMARY
          1. Provide pocket door tracks and hardware systems.
          2. Related Sections: Coordinate with the following as applicable:

Section 087100 – Door Hardware for door hardware not specified in this Section.

Section 087111 – Exposed Track and Hardware Sliding Door Systems.

Section 087112 – Catch’N’Close Sliding Door Hardware.

Section 087113 – Under Glass Sliding Door Systems.

* + - 1. SUBMITTALS
         1. Product Data: Submit manufacturer's literature including product characteristics and accessories.
         2. Shop Drawings: Submit details of construction and mounting.

Provide templates for hardware preparation of doors and frames to be performed in factory.

* + - * 1. Door Hardware Schedule: Comply with scheduling sequence and vertical format in DHI's "Sequence and Format for the Hardware Schedule." Coordinate the final Door Hardware Schedule with doors, frames, and related work to ensure proper size, thickness, hand, function, and finish of door hardware.
        2. Verification Samples: Submit samples of materials selected for use to verify color and finish.
        3. Closeout Submittals:

Operation and Maintenance Data.

Provide any specialized tools required for Owner’s adjustments.

* + - 1. QUALITY ASSURANCE
         1. Manufacturer: Minimum of 5 years experience manufacturing similar products.
         2. Installer: Minimum of 2 years experience installing similar products.
         3. Field Measurements: To the greatest extent practical, take field measurements prior to fabrication.
      2. DELIVERY, STORAGE AND HANDLING
         1. Deliver materials and products in unopened factory labeled packages. Store and handle in strict compliance with manufacturer's instructions and recommendations.

1. PRODUCTS
   * + 1. MANUFACTURER
          1. Basis-of-Design, Canada Contact: K.N. CROWDER MFG. INC., 1220 Burloak Drive, Burlington, Ontario L7L 6B3. Telephone (905) 315-9788. Toll Free 1-866-999-1KNC (1562). Fax (905) 315-8090. Toll Free Fax 1-800-567-0123.
          2. Basis-of-Design, USA Contact: K.N. CROWDER INC., 210 Eighth Street South Lewiston, New York 14092. Telephone (716) 754-8247. Toll Free 1-866-999-1KNC (1562). Toll Free Fax 1-800-567-0123.
       2. PERFORMANCE REQUIREMENTS
          1. Standards Compliance:

ANSI/ BHMA A156.14 – Sliding and Folding Door Hardware.

ANSI/ DHI A115.IG – Installation Guide for Doors and Hardware.

American with Disabilities Act (ADA) 2010 Standards for Accessible Design.

ANSI A117.1 Accessibility Guidelines for Building and Facilities.

All state and local accessibility standards.

* + - * 1. Operating hardware shall be fully exposed and usable from both sides at all times.
        2. Doors shall comply with maximum opening force of 5 lbf applied parallel to door at latch.
      1. pocket door HARDWARE
         1. Catch’N’Close Pocket Door Kit: TYPE CC-W-2X6 Catch’N’Close Crowderframe Pocket Door Kit by K.N. Crowder Inc. with the following characteristics:

Features: Roll formed steel uprights, quick installation, Catch’N’Close system: prevents bouncing and slamming of doors, in-track adjustable stops, nylon wheels with precision ground ball bearings, bottom guide system

Hanger: CC-493: Easy connect Catch’N’Close hanger

Header Track, CC-426: Extruded aluminum, 6063 Alloy, 3 inch (76.2 mm) x 2-19/32 inch (66.1 mm) track

Uprights: Rolled formed steel, 1-1/4 inch (31.8 mm) thick

Load Capacity: up to 150 lbs. (68.0 kg)

Door Thickness: 1-3/4 to 2-1/2 inches (44.5 to 63.5 mm)

Catch’N’Close Capacity: **Choose 1 option: [CC-75 for 75lbs doors] [CC-1 for 150lbs doors]**

Kit Code: **Choose 1 option: NOTE: kit code is based on door size being used, please review the options below and choose the one best suited**

**[TYPE CC-W-2X6 for door width of: 30 to 36 inches (762 to 914 mm) x door height of: 79 to 84 inches (2007 to 2150 mm)]**

**[TYPE CC-W-2X6-EXH8 for door width of: 30 to 36 inches (762 to 914 mm) x door height of: 91 to 96 inches (2311 to 2455 mm)]**

**[TYPE CC-W-2X6-EXH10 for door width of: 30 to 36 inches (762 to 914 mm) x door height of: 115 to 120 inches (2921 to 3064 mm)]**

**[TYPE CC-W-2X6-EXW4 for door width of: greater than 36 to 48 inches (914 to 1219 mm) x door height of: 79 to 84 inches (2007 to 2150 mm)]**

**[TYPE CC-W-2X6-EXW4H8 for door width of: greater than 36 to 48 inches (914 to 1219 mm) x door height of: 91 to 96 inches (2311 to 2455 mm)]**

**[TYPE CC-W-2X6-EXW4H10 for door width of: greater than 36 to 48 inches (914 to 1219 mm) x door height of: 115 to 120 inches (2921 to 3064 mm)]**

**[TYPE CC-NRW-2X6 for door width of: 18 to less than 30 inches (457 to 762 mm) x door height of: 79 to 84 inches (2007 to 2150 mm)]**

**[TYPE CC-NRW-2X6-EXH8 for door width of: 18 to less than 30 inches (457 to 762 mm) x door height of: 91 to 96 inches (2311 to 2455 mm)]**

**[TYPE CC-NRW-2X6-EXH10 for door width of: 18 to less than 30 inches (457 to 762 mm) x door height of: 115 to 120 inches (2921 to 3064 mm)]**

Guide Channel: C-914: 1 inch (25.4 mm) x 29/32 inch (22.9 mm), recessed into bottom of door. Finish Standard Mill

Guide: CP-913 pocket guide

Wall Construction: 2X6 wall construction

Door Application: **Choose 1 option: NOTE: two pocket door kits required for use with one CPD-2X6-JOINER [Standard Single Pocket Door] [Optional Double Bi-Parting Pocket Doors – add CPD-2X6-JOINER kit]**

1. EXECUTION
   * + 1. EXAMINATION
          1. Examine substrates for compliance with requirements for installation tolerances and other conditions affecting performance. Proceed with installation only after unsatisfactory conditions have been corrected.
       2. PREPARATION
          1. Steel Doors and Frames: Comply with ANSI/ BHMA A156-115.
          2. Wood Doors: Comply with ANSI/ BHMA A156-115W.
       3. INSTALLATION
          1. Install products in strict accordance with manufacturer’s instructions, approved submittals and in proper relationship with adjacent construction.
          2. Mounting Heights: Mount door hardware units at heights indicated in the following applicable publications, unless specifically indicated or required to comply with governing regulations:

Standard Steel Doors and Frames: DHI's "Recommended Locations for Architectural Hardware for Standard Steel Doors and Frames."

Custom Steel Doors and Frames: DHI's "Recommended Locations for Builders' Hardware for Custom Steel Doors and Frames."

Wood Doors: DHI WDHS.3, "Recommended Locations for Architectural Hardware for Wood Flush Doors."

* + - * 1. Test for proper operation and adjust until satisfactory results are obtained. Replace units which do not operate properly.
      1. CLEANING
         1. Clean surfaces to remove soiling, stains, dust, and dirt using materials acceptable to manufacturer.

END OF SECTION