**NOTES TO SPECIFIER:**

**Review and remove any text in RED before sending.**

**Edit options are typically flagged in the following manner:**

**EDIT – choices need decision or detailed review**

**NOTE – note to specifier regarding selection**

**OPTION – note when there may be an option for the article and/or paragraph**

**[font in brackets] = edit options for consideration**

SECTION 087114

POCKET DOOR HARDWARE

1. GENERAL
	* + 1. SUMMARY
				1. Provide pocket door tracks and hardware systems.
				2. Related Sections: Coordinate with the following as applicable:

Section 087100 – Door Hardware for door hardware not specified in this Section.

Section 087111 – Exposed Track and Hardware Sliding Door Systems.

Section 087112 – Catch’N’Close Sliding Door Hardware.

Section 087113 – Under Glass Sliding Door Systems.

* + - 1. SUBMITTALS
				1. Product Data: Submit manufacturer's literature including product characteristics and accessories.
				2. Shop Drawings: Submit details of construction and mounting.

Provide templates for hardware preparation of doors and frames to be performed in factory.

* + - * 1. Door Hardware Schedule: Comply with scheduling sequence and vertical format in DHI's "Sequence and Format for the Hardware Schedule." Coordinate the final Door Hardware Schedule with doors, frames, and related work to ensure proper size, thickness, hand, function, and finish of door hardware.
				2. Verification Samples: Submit samples of materials selected for use to verify color and finish.
				3. Closeout Submittals:

Operation and Maintenance Data.

Provide any specialized tools required for Owner’s adjustments.

* + - 1. QUALITY ASSURANCE
				1. Manufacturer: Minimum of 5 years experience manufacturing similar products.
				2. Installer: Minimum of 2 years experience installing similar products.
				3. Field Measurements: To the greatest extent practical, take field measurements prior to fabrication.
			2. DELIVERY, STORAGE AND HANDLING
				1. Deliver materials and products in unopened factory labeled packages. Store and handle in strict compliance with manufacturer's instructions and recommendations.
1. PRODUCTS
	* + 1. MANUFACTURER
				1. Basis-of-Design, Canada Contact: K.N. CROWDER MFG. INC., 1220 Burloak Drive, Burlington, Ontario L7L 6B3. Telephone (905) 315-9788. Toll Free 1-866-999-1KNC (1562). Fax (905) 315-8090. Toll Free Fax 1-800-567-0123.
				2. Basis-of-Design, USA Contact: K.N. CROWDER INC., 210 Eighth Street South Lewiston, New York 14092. Telephone (716) 754-8247. Toll Free 1-866-999-1KNC (1562). Toll Free Fax 1-800-567-0123.
			2. PERFORMANCE REQUIREMENTS
				1. Standards Compliance:

ANSI/ BHMA A156.14 – Sliding and Folding Door Hardware.

ANSI/ DHI A115.IG – Installation Guide for Doors and Hardware.

American with Disabilities Act (ADA) 2010 Standards for Accessible Design.

ANSI A117.1 Accessibility Guidelines for Building and Facilities.

All state and local accessibility standards.

* + - * 1. Operating hardware shall be fully exposed and usable from both sides at all times.
				2. Doors shall comply with maximum opening force of 5 lbf applied parallel to door at latch.
			1. pocket door HARDWARE
				1. Trim Kit: CP-TK-2X4 Snap-On Aluminum Crowderframe Pocket Trim Kit by K.N. Crowder Inc. with the following characteristics:

Snap-On Trim Kit: Allows trim to be installed without visible fasteners

For use only with 1-3/4 inch (44.5 mm) thick doors installed in 2x4 wall with 1/2 inch (12.7 mm) gypsum board and with Type CC-W Catch’N’Close Crowderframe Pocket Door Kit series

Trim Clip, CP-TK-C2X4: Extruded aluminum, 6063 alloy, standard mill finish

Inside Trim Cover, CP-TK-TA2X4: extruded aluminum, 6063 alloy
**Choose 1 finish: [Standard Clear Anodized] [Optional: Bronze Anodized] [Optional: Black Anodized**]

Trim Cover Casing, CP-TK-TC2X4: extruded aluminum, 6063 alloy

**Choose 1 finish: [Standard Clear Anodized] [Optional: Bronze Anodized] [Optional: Black Anodized**]

Bottom Guide Channel, C-917: Recessed in bottom of door, includes pile insert

Kit Code: **Choose 1 option: NOTE: kit code is based on door size being used, please review the options below and choose the one best suited**

**[CP-TK-2X4 Crowderframe Trim Kit for use where a single Type CC-W Catch’N’Close Crowderframe Pocket Door Kit is used. For door width of: 18 to 36 inches (457 to 914 mm) x door height of: 80 to 84 inches (2032 to 2150 mm)]**

**[CP-TK-2X4-EXW4H8 Crowderframe Trim Kit for use where a single Type CC-W-EW4H8 Catch’N’Close Crowderframe Pocket Door Kit is used. For door width of: 36 to 48 inches (914 to 1219 mm) x door height of: 92 to 96 inches (2337 to 2455 mm)]**

**[CPD-TK-2X4 Crowderframe Trim Kit for use where two Type CC-W Catch’N’Close Crowderframe Pocket Door Kits are used with CPD-2X4-JOINER kit. For door widths of: 18 to 36 inches (457 to 914 mm) x door height of: 80 to 84 inches (2032 to 2150 mm) two door applications]**

**[CPD-TK-2X4-EXW4H8 Crowderframe Trim Kit for use where two Type CC-W-EXW4H8 Catch’N’Close Crowderframe Pocket Door Kits are used with CPD-2X4-JOINER kit. For door widths of: 36 to 48 inches (914 to 1219 mm) x door height of: 92 to 96 inches (2337 to 2455 mm) two door applications]**

1. EXECUTION
	* + 1. EXAMINATION
				1. Examine substrates for compliance with requirements for installation tolerances and other conditions affecting performance. Proceed with installation only after unsatisfactory conditions have been corrected.
			2. PREPARATION
				1. Steel Doors and Frames: Comply with ANSI/ BHMA A156-115.
				2. Wood Doors: Comply with ANSI/ BHMA A156-115W.
			3. INSTALLATION
				1. Install products in strict accordance with manufacturer’s instructions, approved submittals and in proper relationship with adjacent construction.
				2. Mounting Heights: Mount door hardware units at heights indicated in the following applicable publications, unless specifically indicated or required to comply with governing regulations:

Standard Steel Doors and Frames: DHI's "Recommended Locations for Architectural Hardware for Standard Steel Doors and Frames."

Custom Steel Doors and Frames: DHI's "Recommended Locations for Builders' Hardware for Custom Steel Doors and Frames."

Wood Doors: DHI WDHS.3, "Recommended Locations for Architectural Hardware for Wood Flush Doors."

* + - * 1. Test for proper operation and adjust until satisfactory results are obtained. Replace units which do not operate properly.
			1. CLEANING
				1. Clean surfaces to remove soiling, stains, dust, and dirt using materials acceptable to manufacturer.

END OF SECTION